
CPP Remote Control Example

1. Create and add a new project-console application.
2. Copy the file to the project root directory.



1. Add the header files (CSerialPort.h,HDP135VExport.h) to the project.
2. Project Properties -> Connector -> Input -> Additional Dependent Projects. Add HDP135VLib.lib.
3. Write the calling code in the main function of the program.



1. Compile to generate executable program.